MATERIAL SAFETY DATA SHEET

SECTION 1	 PRODUCT AND COMPANY IDENTIFICATION	
PRODUCT
Product Name:    DIESEL
Product Description:	   Hydrocarbons and Additives
Product Code: 		   152017-85,   166009-85,   169854-85,   169938-85,   179200-85,   708095-85,   708122-85,   929893-85
Intended Use:  		 Diesel engine fuel

Trade Names	Trade Names	
ADO	 ADO WITH BIOCIDE	
AUTOMOTIVE DIESEL FUEL	 AUTOMOTIVE DIESEL FUEL (ADO)	
AUTOMOTIVE DIESEL FUEL WITH BIOCIDE	 DIESEL (10ppmS) WITH BIOCIDE	
DIESEL WITH BIOCIDE	 LOW SULPHUR DIESEL	
MOBIL DIESEL	 ULSADO	
ULSADO 10ppm BULK (98FJ22)	 ULTRA LOW SULPHUR DIESEL	
ULTRA LOW SULPHUR DIESEL (10ppm S)	 ULTRA LOW SULPHUR DIESEL WITH BIOCIDE	

COMPANY IDENTIFICATION
Supplier:		MOBIL OIL AUSTRALIA PTY LTD 
 A.B.N. 88 004 052 984
12 Riverside Quay  
Southbank
Victoria  3006     Australia 

 24 Hour Environmental / Health Emergency Telephone	 1-800-023-005	
 Product Technical Information	 1-800-033-863	
 Supplier General Contact	 1-800-631-296	

SECTION 2	 HAZARDS IDENTIFICATION	

HAZARD CLASSIFICATION:  HAZARDOUS SUBSTANCE.  NON-DANGEROUS GOOD.

Classified in accordance with Approved Criteria for Classifying Hazardous Substances NOHSC:1008 & according to Australian Dangerous Goods Code.

CLASSIFICATION:    |    Carc. Cat. 3; R40  |    Xn; R20  |    Xn; R65  |    Xi; R38  |  

POISON SCHEDULE NUMBER:   S5 

AS1940 COMBUSTIBLE CLASS:  C1

PHYSICAL / CHEMICAL HAZARDS
   Material can release vapours that readily form flammable mixtures. Vapour accumulation could flash and/or explode if ignited.   Material can accumulate static charges which may cause an ignition.

HEALTH HAZARDS
 Limited evidence of a carcinogenic effect.  Harmful by inhalation.  Harmful: may cause lung damage if swallowed.  Irritating to skin.  Under conditions of poor personal hygiene and prolonged repeated contact, some polycyclic aromatic compounds (PACs) have been suspected as a cause of skin cancer in humans.  May be irritating to the eyes, nose, throat, and lungs.  High-pressure injection under skin may cause serious damage.

ENVIRONMENTAL HAZARDS
 Toxic to aquatic organisms, may cause long-term adverse effects in the aquatic environment.

SAFETY PHRASE(S):  S2; Keep out of the reach of children.  S36/37; Wear suitable protective clothing and gloves.  S61; Avoid release to the environment. Refer to special instructions/safety data sheets.  S62; If swallowed, do not induce vomiting: seek medical advice immediately and show this container or label.
 
NOTE:   This material should not be used for any other purpose than the intended use in Section 1 without expert advice. Health studies have shown that chemical exposure may cause potential human health risks which may vary from person to person. 

 SECTION 3	 COMPOSITION / INFORMATION ON INGREDIENTS	
 
This material is regulated as a preparation.

Reportable Hazardous Substance(s) or Complex Substance(s) 
 Name	 CAS#	 Concentration*	 Symbols/Risk Phrases	
 FUELS, DIESEL	 68334-30-5	 > 99 %	 Xn;R20, Xi;R38, Xn;Carc. Cat. 3;R40, Xn;R65	
    
 * All concentrations are percent by weight unless ingredient is a gas. Gas concentrations are in percent by volume.

NOTE:  Composition may contain up to 0.5% performance additives and / or dyes. Other ingredients determined not to be hazardous up to 100%.

 SECTION 4	 FIRST AID MEASURES	

INHALATION
Remove from further exposure.  For those providing assistance, avoid exposure to yourself or others.  Use adequate respiratory protection.  If respiratory irritation, dizziness, nausea, or unconsciousness occurs, seek immediate medical assistance.  If breathing has stopped, assist ventilation with a mechanical device or use mouth-to-mouth resuscitation.

SKIN CONTACT
Remove contaminated clothing.  Dry wipe exposed skin and cleanse with waterless hand cleaner and follow by washing thoroughly with soap and water.  For those providing assistance, avoid further skin contact to yourself or others.  Wear impervious gloves.  Launder contaminated clothing separately before reuse.  Discard contaminated articles that cannot be laundered.  If product is injected into or under the skin, or into any part of the body, regardless of the appearance of the wound or its size, the individual should be evaluated immediately by a physician as a surgical emergency. Even though initial symptoms from high pressure injection may be minimal or absent, early surgical treatment within the first few hours may significantly reduce the ultimate extent of injury.

EYE CONTACT
Flush thoroughly with water.  If irritation occurs, get medical assistance.

INGESTION
Seek immediate medical attention.  Do not induce vomiting.

NOTE TO PHYSICIAN
If ingested, material may be aspirated into the lungs and cause chemical pneumonitis.  Treat appropriately.

PRE-EXISTING MEDICAL CONDITIONS WHICH MAY BE AGGRAVATED BY EXPOSURE
Contains hydrocarbon solvent/petroleum hydrocarbons;  skin contact may aggravate an existing dermatitis. 

SECTION 5	FIRE FIGHTING MEASURES	

EXTINGUISHING MEDIA
Appropriate Extinguishing Media:  Use water fog, foam, dry chemical or carbon dioxide (CO2) to extinguish flames.

Inappropriate Extinguishing Media:  Straight streams of water

FIRE FIGHTING
Fire Fighting Instructions:  Evacuate area.  Prevent run-off from fire control or dilution from entering streams, sewers or drinking water supply.  Fire-fighters should use standard protective equipment and in enclosed spaces, self-contained breathing apparatus (SCBA).   Use water spray to cool fire exposed surfaces and to protect personnel.  

Hazardous Combustion Products:   Smoke, Fume, Aldehydes, Sulphur oxides, Incomplete combustion products, Oxides of carbon

FLAMMABILITY PROPERTIES 
Flash Point [Method]:  64°C  (147°F)  [ASTM D-93]
Flammable Limits (Approximate volume % in air):   LEL:  0.6     UEL: 7.0
Autoignition Temperature:  N/D 

 SECTION 6	 ACCIDENTAL RELEASE MEASURES	

NOTIFICATION PROCEDURES
In the event of a spill or accidental release, notify relevant authorities in accordance with all applicable regulations.

PROTECTIVE MEASURES
Avoid contact with spilled material.  Warn or evacuate occupants in surrounding and downwind areas if required, due to toxicity or flammability of the material.  See Section 5 for fire fighting information.  See the Hazard Identification Section for Significant Hazards.  See Section 4 for First Aid Advice.  See Section 8 for advice on the minimum requirements for personal protective equipment. Additional protective measures may be necessary, depending on the specific circumstances and/or the expert judgment of the emergency responders.  For emergency responders:  Respiratory protection: half-face or full-face respirator with filter(s) for organic vapor and, when applicable, H2S, or Self Contained Breathing Apparatus (SCBA) can be used depending on the size of spill and potential level of exposure.  If the exposure cannot be completely characterized or an oxygen deficient atmosphere is possible or anticipated, SCBA is recommended.   Work gloves that are resistant to aromatic hydrocarbons are recommended.  Note: gloves made of polyvinyl acetate (PVA) are not water-resistant and are not suitable for emergency use.  Chemical goggles are recommended if splashes or contact with eyes is possible.  Small spills: normal antistatic work clothes are usually adequate.  Large spills: full body suit of chemical resistant, antistatic material is recommended.
 
SPILL MANAGEMENT
Land Spill:  Eliminate all ignition sources (no smoking, flares, sparks or flames in immediate area).  Stop leak if you can do so without risk.  All equipment used when handling the product must be grounded.  Do not touch or walk through spilled material.  Prevent entry into waterways, sewer, basements or confined areas.  A vapour-suppressing foam may be used to reduce vapour.  Use clean non-sparking tools to collect absorbed material.  Absorb or cover with dry earth, sand or other non-combustible material and transfer to containers.  Large Spills:  Water spray may reduce vapour, but may not prevent ignition in enclosed spaces.

Water Spill:  Stop leak if you can do so without risk.  Confine the spill immediately with booms.  Warn other shipping.  Remove from the surface by skimming or with suitable absorbents.  Seek the advice of a specialist before using dispersants.

Water spill and land spill recommendations are based on the most likely spill scenario for this material; however, geographic conditions, wind, temperature, (and in the case of a water spill) wave and current direction and speed may greatly influence the appropriate action to be taken.  For this reason, local experts should be consulted.  Note:  Local regulations may prescribe or limit action to be taken. 

ENVIRONMENTAL PRECAUTIONS
Large Spills:  Dyke far ahead of liquid spill for later recovery and disposal.  Prevent entry into waterways, sewers, basements or confined areas.

 SECTION 7	HANDLING AND STORAGE	

HANDLING
Avoid all personal contact.  Do not siphon by mouth. Do not use as a cleaning solvent or other non-motor fuel uses.  For use as a motor fuel only.  It is dangerous and/or unlawful to put petrol into unapproved containers. Do not fill container while it is in or on a vehicle. Static electricity may ignite vapour and cause fire. Place container on ground when filling and keep nozzle in contact with container.  Do not use electronic devices (including but not limited to cellular phones, computers, calculators, pagers or other electronic devices etc) in or around any fuelling operation or storage area unless the devices are certified intrinsically safe by an approved national testing agency and to the safety standards required by national and/or local laws and regulations.  Prevent small spills and leakage to avoid slip hazard.   Material can accumulate static charges which may cause an electrical spark (ignition source).  When the material is handled in bulk, an electrical spark could ignite any flammable vapors from liquids or residues that may be present (e.g., during switch-loading operations).  Use proper bonding and/or earthing procedures.  However, bonding and earthing may not eliminate the hazard from static accumulation.  Consult local applicable standards for guidance.  Additional references include American Petroleum Institute 2003 (Protection Against Ignitions Arising out of Static, Lightning and Stray Currents) or National Fire Protection Agency 77 (Recommended Practice on Static Electricity) or CENELEC CLC/TR 50404 (Electrostatics - Code of practice for the avoidance of hazards due to static electricity).    

Static Accumulator:   This material is a static accumulator.  A liquid is typically considered a nonconductive, static accumulator if its conductivity is below 100 pS/m (100x10E-12 Siemens per meter) and is considered a semiconductive, static accumulator if its conductivity is below 10,000 pS/m.  Whether a liquid is nonconductive or semiconductive, the precautions are the same.  A number of factors, for example liquid temperature, presence of contaminants, anti-static additives and filtration can greatly influence the conductivity of a liquid.

STORAGE
The container choice, for example storage vessel, may effect static accumulation and dissipation.  Keep container closed. Handle containers with care. Open slowly in order to control possible pressure release.  Store in a cool, well-ventilated area.  Storage containers should be earthed and bonded.  Fixed storage containers, transfer containers and associated equipment should be earthed and bonded to prevent accumulation of static charge.           

Material is defined under the National Standard [NOHSC:1015] Storage and Handling of Workplace Dangerous Goods.

 SECTION 8	 EXPOSURE CONTROLS / PERSONAL PROTECTION	

EXPOSURE LIMIT VALUES

Exposure limits/standards (Note: Exposure limits are not additive)

 Substance Name	Form	Limit/Standard	Note	Source	Year	
FUELS, DIESEL	Stable Aerosol.	TWA	5 mg/m3			ExxonMobil	2010	
FUELS, DIESEL	Vapour.	TWA	200 mg/m3			ExxonMobil	2010	
FUELS, DIESEL [total hydrocarb, vapor&aerosol]	Inhalable fraction and vapour	TWA	100 mg/m3		Skin	ACGIH	2011	

NOTE: Limits/standards shown for guidance only.  Follow applicable regulations.

Biological limits
 
No biological limits allocated.

ENGINEERING CONTROLS

The level of protection and types of controls necessary will vary depending upon potential exposure conditions.  Control measures to consider:
 Use explosion-proof ventilation equipment to stay below exposure limits.

PERSONAL PROTECTION
 
Personal protective equipment selections vary based on potential exposure conditions such as applications, handling practices, concentration and ventilation.  Information on the selection of protective equipment for use with this material, as provided below, is based upon intended, normal usage.  

Respiratory Protection:   If engineering controls do not maintain airborne contaminant concentrations at a level which is adequate to protect worker health, an approved respirator may be appropriate.  Respirator selection, use, and maintenance must be in accordance with regulatory requirements, if applicable.  Types of respirators to be considered for this material include: 
Organic vapour
No special requirements under ordinary conditions of use and with adequate ventilation. 

For high airborne concentrations, use an approved supplied-air respirator, operated in positive pressure mode.  Supplied air respirators with an escape bottle may be appropriate when oxygen levels are inadequate, gas/vapour warning properties are poor, or if air purifying filter capacity/rating may be exceeded.

Hand Protection:   Any specific glove information provided is based on published literature and glove manufacturer data.  Glove suitability and breakthrough time will differ depending on the specific use conditions. Contact the glove manufacturer for specific advice on glove selection and breakthrough times for your use conditions. Inspect and replace worn or damaged gloves. The types of gloves to be considered for this material include:
Nitrile,Viton
Chemical resistant gloves are recommended. If contact with forearms is likely wear gauntlet style gloves.

Eye Protection:   If contact with material is likely, chemical goggles are recommended.

Skin and Body Protection:    Any specific clothing information provided is based on published literature or manufacturer data.  The types of clothing to be considered for this material include:
 Chemical/oil resistant clothing is recommended.

Specific Hygiene Measures:   Always observe good personal hygiene measures, such as washing after handling the material and before eating, drinking, and/or smoking. Routinely wash work clothing and protective equipment to remove contaminants. Discard contaminated clothing and footwear that cannot be cleaned. Practise good housekeeping.

ENVIRONMENTAL CONTROLS
 Comply with applicable environmental regulations limiting discharge to air, water and
soil. Protect the environment by applying appropriate control measures to prevent or limit
emissions.

SECTION 9	 PHYSICAL AND CHEMICAL PROPERTIES	

Note:  Physical and chemical properties are provided for safety, health and environmental considerations only and may not fully represent product specifications.  Contact the Supplier for additional information.

GENERAL INFORMATION
Physical State:    Liquid 
Colour:   Clear (May Be Dyed)
Odour:   Petroleum/Solvent
Odour Threshold:   N/D

IMPORTANT HEALTH, SAFETY, AND ENVIRONMENTAL INFORMATION
Relative Density (at 15 °C):    0.82 -  0.85    
Flash Point [Method]:     64°C  (147°F)  [ASTM D-93]
Flammable Limits (Approximate volume % in air):   LEL:  0.6     UEL: 7.0  
Autoignition Temperature:  N/D 
Boiling Point / Range:    > 185°C (365°F)
Vapour Density (Air = 1):   > 2 at 101 kPa
Vapour Pressure:    0.067 kPa (0.5 mm Hg) at 20 ºC
Evaporation Rate (n-butyl acetate = 1):   N/D
pH:   N/A
Log Pow (n-Octanol/Water Partition Coefficient):   > 3.5
Solubility in Water:   Negligible
Viscosity:   2 cSt (2 mm2/sec) at 40 ºC - 4.5 cSt  (4.5 mm2/sec) at 40 ºC
Oxidizing Properties:  See Hazards Identification Section.

OTHER INFORMATION
Freezing Point:   N/D
Melting Point:   N/A
Pour Point:     < 18°C  (64°F)      

 SECTION 10	 STABILITY AND REACTIVITY	

STABILITY:  Material is stable under normal conditions.

CONDITIONS TO AVOID:  Open flames and high energy ignition sources.

INCOMPATIBLE MATERIALS:   Halogens,  Alkalies,  Strong Acids,  Strong oxidisers

HAZARDOUS DECOMPOSITION PRODUCTS:  Material does not decompose at ambient temperatures.

HAZARDOUS REACTIONS:  Will not occur.

SECTION 11	 TOXICOLOGICAL INFORMATION	

ACUTE TOXICITY

 Route of Exposure	 Conclusion / Remarks	
Inhalation		
Toxicity (Rat): LC50 > >4000 mg/m3	Moderately toxic. Based on test data for structurally similar materials.	
Irritation: Data available.	Elevated temperatures or mechanical action may form vapours, mist, or fumes which may be irritating to the eyes, nose, throat, or lungs. Based on test data for structurally similar materials.	
		
Ingestion		
Toxicity (Rat): LD50 > 5000 mg/kg	Minimally Toxic. Based on test data for structurally similar materials.	
		
Skin		
Toxicity (Rabbit): LD50 > 5000 mg/kg	Minimally Toxic. Based on test data for structurally similar materials.	
Irritation (Rabbit): Data available.	Irritating to the skin. Based on test data for structurally similar materials.	
		
Eye 		
Irritation (Rabbit): Data available.	May cause mild, short-lasting discomfort to eyes. Based on test data for structurally similar materials.	

CHRONIC/OTHER EFFECTS
             For the product itself:
 Vapour concentrations above recommended exposure levels are irritating to the eyes and the respiratory tract, may cause headaches and dizziness, are anaesthetic and may have other central nervous system effects.  Small amounts of liquid aspirated into the lungs during ingestion or from vomiting may cause chemical pneumonitis or pulmonary edema.
Diesel fuel:  Carcinogenic in animal tests. Caused mutations in-vitro.  Repeated dermal exposures to high concentrations in test animals resulted in  reduced litter size and litter weight, and increased fetal resorptions at maternally toxic doses. Dermal exposure to high concentrations resulted in severe skin irritation with weight loss and some mortality. Inhalation exposure to high concentrations resulted in respiratory tract irritation, lung changes/infiltration/accumulation, and reduction in lung function.  Diesel exhaust fumes:  Carcinogenic in animal tests. Inhalation exposures to exhaust for 2 years in test animals resulted in lung tumours and lymphoma. Extract of particulate produced skin tumours in test animals.  Caused mutations in-vitro.

Additional information is available by request.
 
IARC Classification:
The following ingredients are cited on the lists below:  None.

--REGULATORY LISTS SEARCHED--	
 1 = IARC 1	 2 = IARC 2A	 3 = IARC 2B	

 SECTION 12	 ECOLOGICAL INFORMATION	

The information given is based on data available for the material, the components of the material, and similar materials.

ECOTOXICITY   
             Material -- Expected to be toxic to aquatic organisms. May cause long-term adverse effects in the aquatic environment.

MOBILITY 
             More volatile component -- Highly volatile, will partition rapidly to air.  Not expected to partition to sediment and wastewater solids.
             High molecular wt. component -- Low solubility and floats and is expected to migrate from water to the land.  Expected to partition to sediment and wastewater solids. 

PERSISTENCE AND DEGRADABILITY
Biodegradation: 
             Majority of components --  Expected to be inherently biodegradable  
Atmospheric Oxidation: 
             More volatile component -- Expected to degrade rapidly in air

BIOACCUMULATION POTENTIAL 
             Base oil component -- Has the potential to bioaccumulate, however metabolism or physical properties may reduce the bioconcentration or limit bioavailability.

    

 

 
 SECTION 13	 DISPOSAL CONSIDERATIONS	
 
Disposal recommendations based on material as supplied.  Disposal must be in accordance with current applicable laws and regulations, and material characteristics at time of disposal. 

DISPOSAL RECOMMENDATIONS
 Product is suitable for burning in an enclosed controlled burner for fuel value or disposal by supervised incineration at very high temperatures to prevent formation of undesirable combustion products. 
 
 Empty Container Warning Empty Container Warning (where applicable):  Empty containers may contain residue and can be dangerous.  Do not attempt to refill or clean containers without proper instructions.  Empty drums should be completely drained and safely stored until appropriately reconditioned or disposed.  Empty containers should be taken for recycling, recovery, or disposal through suitably qualified or licensed contractor and in accordance with governmental regulations.  DO NOT PRESSURISE, CUT, WELD, BRAZE, SOLDER, DRILL, GRIND, OR EXPOSE SUCH CONTAINERS TO HEAT, FLAME, SPARKS, STATIC ELECTRICITY, OR OTHER SOURCES OF IGNITION.  THEY MAY EXPLODE AND CAUSE INJURY OR DEATH.

 SECTION 14	 TRANSPORT INFORMATION	
LAND (ADG) :  Not Regulated for Land Transport

Footnote:  Special Provision AU02 applies if shipped in one or more compartments of a tank vehicle or portable tank transporting other refined petroleum products.

SEA (IMDG) 
Proper Shipping Name:   ENVIRONMENTALLY HAZARDOUS SUBSTANCES, LIQUID, N.O.S.
Hazard Class & Division:    9
EMS Number:   F-A, S-F
UN Number:   3082
Packing Group:   III
Marine Pollutant:   Yes
Label(s):   9
Transport Document Name:      UN3082, ENVIRONMENTALLY HAZARDOUS SUBSTANCES, LIQUID, N.O.S., 9, PG III, MARINE POLLUTANT (Fuels, diesel)

AIR (IATA) 
Proper Shipping Name:   ENVIRONMENTALLY HAZARDOUS SUBSTANCES, LIQUID, N.O.S. (Fuels, diesel)
Hazard Class & Division:   9 
UN Number:   3082
Packing Group:   III
Label(s) / Mark(s):   9, EHS   
Transport Document Name:    UN3082, ENVIRONMENTALLY HAZARDOUS SUBSTANCES, LIQUID, N.O.S. (Fuels, diesel), 9, PG III

 SECTION 15	 REGULATORY INFORMATION	
 
Material is hazardous as defined by the Approved Criteria for Classifying Hazardous Substances NOHSC:1008.

CLASSIFICATION:   Category 3 Carcinogen.  Harmful.  Irritant. The classification of this product is based all or in part on test data. 

Nature of Special Risk:  R40; Limited evidence of a carcinogenic effect.  R20; Harmful by inhalation.  R65; Harmful: may cause lung damage if swallowed.  R38; Irritating to skin.

SAFETY PHRASE(S):  S2; Keep out of the reach of children.  S36/37; Wear suitable protective clothing and gloves.  S61; Avoid release to the environment. Refer to special instructions/safety data sheets.  S62; If swallowed, do not induce vomiting: seek medical advice immediately and show this container or label.

Contains:  FUELS, DIESEL   

Product is not regulated according to Australian Dangerous Goods Code. 

Poison Schedule number allocated by the Standard for the Uniform Scheduling of Medicines and Poisons (SUSMP) established under the Therapeutic Goods Act.

REGULATORY STATUS AND APPLICABLE LAWS AND REGULATIONS

Complies with the following national/regional chemical inventory requirements:   EINECS, PICCS, TSCA, AICS

 SECTION 16	 OTHER INFORMATION	

KEY TO ABBREVIATIONS AND ACRONYMS:
N/D = Not determined, N/A = Not applicable, STEL = Short-Term Exposure Limit, TWA = Time-Weighted Average

KEY TO THE RISK CODES CONTAINED IN SECTION 2 AND 3 OF THIS DOCUMENT (for information only):
 R20; Harmful by inhalation.
R38; Irritating to skin.
R40; Limited evidence of a carcinogenic effect.
R65; Harmful: may cause lung damage if swallowed.

THIS SAFETY DATA SHEET CONTAINS THE FOLLOWING REVISIONS:
 Revision Changes:
Hazard Identification: Health Hazards was modified.
Section 06: Protective Measures was modified.
Section 11: Skin Irritation Conclusion was modified.
Section 09: Phys/Chem Properties Note was modified.
Section 11: Inhalation Lethality Conclusion was modified.
Section 09: Boiling Point ºC(ºF) was modified.
Section 08: Comply with applicable regulations phrase was modified.
Section 09: Vapour Pressure was modified.
Section 11: Inhalation Lethality Test Data was modified.
Section 09: Relative Density - Header was modified.
Section 09: Flash Point ºC(ºF) was modified.
Section 09: Viscosity was modified.
Section 04: First Aid Pre-existing Medical Conditions was modified.
Section 08: Skin and Body Protection was modified.
Section 15: National Chemical Inventory Listing was modified.
Hazard Identification: Classification was modified.
Section 15: Classification was modified.
Composition: Component Table was modified.
Section 15: NATURE OF SPECIAL RISK was modified.
Section 16: RCode Key was modified.
Section 08: Exposure Limits Table was modified.
Section 15: Australian Poison Schedule Allocated was modified.
Section 01: Alternate Product Names Table was added.
Section 01: Alternate Product Name Header was added.

  
THIS SDS COVERS THE FOLLOWING MATERIALS:  ADO  |  ADO WITH BIOCIDE  |  AUTOMOTIVE DIESEL FUEL  |  AUTOMOTIVE DIESEL OIL (ADO)  |  AUTOMOTIVE DIESEL WITH BIOCIDE  |  DIESEL (10ppmS) WITH BIOCIDE  |  DIESEL WITH BIOCIDE  |  LOW SULPHUR DIESEL  |  MOBIL DIESEL  |  ULSADO  |  ULSADO 10ppm BULK (98FJ22)  |  ULTRA LOW SULPHUR DIESEL  |  ULTRA LOW SULPHUR DIESEL (10ppm S)  |  ULTRA LOW SULPHUR DIESEL WITH BIOCIDE
 -----------------------------------------------------------------------------------------------------------------------------------------------------
 The information and recommendations contained herein are, to the best of ExxonMobil's knowledge and belief, accurate and reliable as of the date issued.  You can contact ExxonMobil to insure that this document is the most current available from ExxonMobil.  The information and recommendations are offered for the user's consideration and examination.  It is the user's responsibility to satisfy itself that the product is suitable for the intended use.  If buyer repackages this product, it is the user's responsibility to insure proper health, safety and other necessary information is included with and/or on the container.  Appropriate warnings and safe-handling procedures should be provided to handlers and users.  Alteration of this document is strictly prohibited.  Except to the extent required by law, re-publication or retransmission of this document, in whole or in part, is not permitted.  The term, "ExxonMobil" is used for convenience, and may include any one or more of ExxonMobil Chemical Company, Exxon Mobil Corporation, or any affiliates in which they directly of indirectly hold any interest.

 -----------------------------------------------------------------------------------------------------------------------------------------------------
DGN:  2000461XAU  (1011103)
-----------------------------------------------------------------------------------------------------------------------------------------------------
 Prepared by:          Exxon Mobil Corporation
                              EMBSI, Clinton NJ USA
Contact Point:       See Section 1 for Local Contact number

End of (M)SDS