MATERIAL SAFETY DATA SHEET

SECTION 1	 PRODUCT AND COMPANY IDENTIFICATION	
PRODUCT
Product Name:    HOME KEROSENE / DUAL PURPOSE KEROSENE
Product Description:	   Petroleum Hydrocarbons
Product Code: 		   136028-85
Intended Use:  		 Fuel

COMPANY IDENTIFICATION
Supplier:		Just Fuel Petroleum Services Pty Ltd
                      2 Western Avenue Sunshine Vic 3020

 24 Hour Environmental / Health Emergency Telephone	 03 9312 4788	
 Product Technical Information	 1-800-033-863	
 Supplier General Contact	 1-800-631-296	

SECTION 2	 HAZARDS IDENTIFICATION	

HAZARD CLASSIFICATION:  HAZARDOUS SUBSTANCE.  DANGEROUS GOOD.

Classified in accordance with Approved Criteria for Classifying Hazardous Substances NOHSC:1008 & according to Australian Dangerous Goods Code.

CLASSIFICATION:    |    Carc. Cat. 3; R40  |    Xn; R65  |    Xi; R38  |  

POISON SCHEDULE NUMBER:   S5 

PHYSICAL / CHEMICAL HAZARDS
 Flammable.  Material can release vapours that readily form flammable mixtures. Vapour accumulation could flash and/or explode if ignited.   Material can accumulate static charges which may cause an ignition.

HEALTH HAZARDS
 Limited evidence of a carcinogenic effect.  Harmful: may cause lung damage if swallowed.  Irritating to skin.  May be irritating to the eyes, nose, throat, and lungs.  Breathing of high vapour concentrations may cause dizziness, light-headedness, headache, nausea and loss of co-ordination.  Continued inhalation may result in unconsciousness.  High-pressure injection under skin may cause serious damage.

ENVIRONMENTAL HAZARDS
 Toxic to aquatic organisms, may cause long-term adverse effects in the aquatic environment.

SAFETY PHRASE(S):  S2; Keep out of the reach of children.  S23; Do not breathe vapour.  S24; Avoid contact with skin.  S36/37; Wear suitable protective clothing and gloves.  S43; In case of fire use carbon dioxide (CO2), foam, dry chemical, or water fog.  S61; Avoid release to the environment. Refer to special instructions/safety data sheets.  S62; If swallowed, do not induce vomiting: seek medical advice immediately and show this container or label.
 
NOTE:   This material should not be used for any other purpose than the intended use in Section 1 without expert advice. Health studies have shown that chemical exposure may cause potential human health risks which may vary from person to person. 

 SECTION 3	 COMPOSITION / INFORMATION ON INGREDIENTS	
 
This material is regulated as a complex substance.

Reportable Hazardous Substance(s) or Complex Substance(s) 
 Name	 CAS#	 Concentration*	 Symbols/Risk Phrases	
 KEROSENE	 8008-20-6	 100%	 R10, Xi;R38, Xn;Carc. Cat. 3;R40, Xn;R65	
  
Reportable Hazardous Constituent(s) Contained in Complex Substance(s) 
 Name	 CAS#	 Concentration*	 Symbols/Risk Phrases	
 NAPHTHALENE	 91-20-3	 < 2%	 Xn;R22, Xn;Carc. Cat. 3;R40	
 ETHYL BENZENE	 100-41-4	 0.1 - 1%	 F;R11, Xn;R20	
  
 * All concentrations are percent by weight unless ingredient is a gas. Gas concentrations are in percent by volume. Other ingredients determined not to be hazardous up to 100%.

 SECTION 4	 FIRST AID MEASURES	

INHALATION
Remove from further exposure.  For those providing assistance, avoid exposure to yourself or others.  Use adequate respiratory protection.  If respiratory irritation, dizziness, nausea, or unconsciousness occurs, seek immediate medical assistance.  If breathing has stopped, assist ventilation with a mechanical device or use mouth-to-mouth resuscitation.

SKIN CONTACT
Wash contact areas with soap and water.  Remove contaminated clothing.  Launder contaminated clothing before reuse.  If product is injected into or under the skin, or into any part of the body, regardless of the appearance of the wound or its size, the individual should be evaluated immediately by a physician as a surgical emergency. Even though initial symptoms from high pressure injection may be minimal or absent, early surgical treatment within the first few hours may significantly reduce the ultimate extent of injury.

EYE CONTACT
Flush thoroughly with water.  If irritation occurs, get medical assistance.

INGESTION
Seek immediate medical attention.  Do not induce vomiting.

NOTE TO PHYSICIAN
If ingested, material may be aspirated into the lungs and cause chemical pneumonitis.  Treat appropriately.

PRE-EXISTING MEDICAL CONDITIONS WHICH MAY BE AGGRAVATED BY EXPOSURE
Hydrocarbon Solvents/Petroleum Hydrocarbons- Skin contact may aggravate an existing dermatitis. 

SECTION 5	FIRE FIGHTING MEASURES	

EXTINGUISHING MEDIA
Appropriate Extinguishing Media:  Use water fog, foam, dry chemical or carbon dioxide (CO2) to extinguish flames.

Inappropriate Extinguishing Media:  Straight streams of water

FIRE FIGHTING
Fire Fighting Instructions:  Evacuate area.  Prevent run-off from fire control or dilution from entering streams, sewers or drinking water supply.  Fire-fighters should use standard protective equipment and in enclosed spaces, self-contained breathing apparatus (SCBA).   Use water spray to cool fire exposed surfaces and to protect personnel. 

Unusual Fire Hazards:  FLAMMABLE.  Hazardous material. Firefighters should consider protective equipment indicated in Section 8.  Vapour is flammable and heavier than air.  Vapour may travel across the ground and reach remote ignition sources, causing a flashback fire danger.

Hazardous Combustion Products:   Smoke, Fume, Aldehydes, Sulphur oxides, Incomplete combustion products, Oxides of carbon

FLAMMABILITY PROPERTIES 
Flash Point [Method]:  >38C  (100F) [ IP 170/70]
Flammable Limits (Approximate volume % in air):   LEL:  0.7     UEL: 5.0
Autoignition Temperature:   250°C  (482°F)

Hazchem Code:   3[Y]

 SECTION 6	 ACCIDENTAL RELEASE MEASURES	

NOTIFICATION PROCEDURES
In the event of a spill or accidental release, notify relevant authorities in accordance with all applicable regulations.

PROTECTIVE MEASURES
Avoid contact with spilled material.  Warn or evacuate occupants in surrounding and downwind areas if required, due to toxicity or flammability of the material.  See Section 5 for fire fighting information.  See the Hazard Identification Section for Significant Hazards.  See Section 4 for First Aid Advice.  See Section 8 for Personal Protective Equipment.
 
SPILL MANAGEMENT
Land Spill:  Eliminate all ignition sources (no smoking, flares, sparks or flames in immediate area).  Stop leak if you can do so without risk.  All equipment used when handling the product must be grounded.  Do not touch or walk through spilled material.  Prevent entry into waterways, sewer, basements or confined areas.  A vapour-suppressing foam may be used to reduce vapour.  Use clean non-sparking tools to collect absorbed material.  Absorb or cover with dry earth, sand or other non-combustible material and transfer to containers.  Large Spills:  Water spray may reduce vapour, but may not prevent ignition in enclosed spaces.

Water Spill:  Stop leak if you can do so without risk.  Eliminate sources of ignition.  Warn other shipping.  If the Flash Point exceeds the Ambient Temperature by 10 deg C or more, use containment booms and remove from the surface by skimming or with suitable absorbents when conditions permit.  If the Flash Point does not exceed the Ambient Air Temperature by at least 10C, use booms as a barrier to protect shorelines and allow material to evaporate.  Seek the advice of a specialist before using dispersants.

Water spill and land spill recommendations are based on the most likely spill scenario for this material; however, geographic conditions, wind, temperature, (and in the case of a water spill) wave and current direction and speed may greatly influence the appropriate action to be taken.  For this reason, local experts should be consulted.  Note:  Local regulations may prescribe or limit action to be taken. 

ENVIRONMENTAL PRECAUTIONS
Large Spills:  Dyke far ahead of liquid spill for later recovery and disposal.  Prevent entry into waterways, sewers, basements or confined areas.

 SECTION 7	HANDLING AND STORAGE	

HANDLING
Avoid all personal contact.  Do not siphon by mouth. It is dangerous and/or unlawful to put petrol into unapproved containers. Do not fill container while it is in or on a vehicle. Static electricity may ignite vapour and cause fire. Place container on ground when filling and keep nozzle in contact with container.  Do not use electronic devices (including but not limited to cellular phones, computers, calculators, pagers or other electronic devices etc) in or around any fuelling operation or storage area unless the devices are certified intrinsically safe by an approved national testing agency and to the safety standards required by national and/or local laws and regulations.  Prevent small spills and leakage to avoid slip hazard.   Material can accumulate static charges which may cause an electrical spark (ignition source).  Use proper bonding and/or ground procedures.  However, bonding and grounds may not eliminate the hazard from static accumulation.  Consult local applicable standards for guidance.  Additional references include American Petroleum Institute 2003 (Protection Against Ignitions Arising out of Static, Lightning and Stray Currents) or National Fire Protection Agency 77 (Recommended Practice on Static Electricity) or CENELEC CLC/TR 50404 (Electrostatics - Code of practice for the avoidance of hazards due to static electricity).    

Static Accumulator:   This material is a static accumulator.  A liquid is typically considered a nonconductive, static accumulator if its conductivity is below 100 pS/m (100x10E-12 Siemens per meter) and is considered a semiconductive, static accumulator if its conductivity is below 10,000 pS/m.  Whether a liquid is nonconductive or semiconductive, the precautions are the same.  A number of factors, for example liquid temperature, presence of contaminants, anti-static additives and filtration can greatly influence the conductivity of a liquid.

STORAGE
The container choice, for example storage vessel, may effect static accumulation and dissipation.  Keep container closed. Handle containers with care. Open slowly in order to control possible pressure release.  Store in a cool, well-ventilated area.  Storage containers should be earthed and bonded.  Fixed storage containers, transfer containers and associated equipment should be earthed and bonded to prevent accumulation of static charge.           

 SECTION 8	 EXPOSURE CONTROLS / PERSONAL PROTECTION	

EXPOSURE LIMIT VALUES

Exposure limits/standards (Note: Exposure limits are not additive)

 Substance Name	Form	Limit/Standard	Note	Source	Year	
ETHYL BENZENE		STEL	543 mg/m3	125 ppm		Australia OELs	2005	
ETHYL BENZENE		TWA	434 mg/m3	100 ppm		Australia OELs	2005	
ETHYL BENZENE		STEL	125 ppm			ACGIH	2009	
ETHYL BENZENE		TWA	100 ppm			ACGIH	2009	
KEROSENE	Stable Aerosol.	TWA	5 mg/m3			ExxonMobil	2009	
KEROSENE	Vapour.	TWA	200 mg/m3			ExxonMobil	2009	
KEROSENE [as total hydrocarbon vapor]	Non-Aerosol	TWA	200 mg/m3		Skin	ACGIH	2009	
NAPHTHALENE		STEL	79 mg/m3	15 ppm		Australia OELs	2005	
NAPHTHALENE		TWA	52 mg/m3	10 ppm		Australia OELs	2005	
NAPHTHALENE		STEL	15 ppm		Skin	ACGIH	2009	
NAPHTHALENE		TWA	10 ppm		Skin	ACGIH	2009	

NOTE: Limits/standards shown for guidance only.  Follow applicable regulations.

Biological limits

Substance Name	Specimen	Sampling Time	Limit	Determinant	Source	
ETHYL BENZENE	End-exhaled air	Not applicable		Ethyl benzene	ACGIH BELs	
ETHYL BENZENE	Urine	End of shift at end of work wk	1.5 g/g creatinine	Mandelic acid	ACGIH BELs	
NAPHTHALENE	Urine	End of shift at end of work wk		1-Hydroxypyrene, with hydrolysis (1-HP)	ACGIH BELs	

ENGINEERING CONTROLS

The level of protection and types of controls necessary will vary depending upon potential exposure conditions.  Control measures to consider:
 Use explosion-proof ventilation equipment to stay below exposure limits.

PERSONAL PROTECTION
 
Personal protective equipment selections vary based on potential exposure conditions such as applications, handling practices, concentration and ventilation.  Information on the selection of protective equipment for use with this material, as provided below, is based upon intended, normal usage.  

Respiratory Protection:   If engineering controls do not maintain airborne contaminant concentrations at a level which is adequate to protect worker health, an approved respirator may be appropriate.  Respirator selection, use, and maintenance must be in accordance with regulatory requirements, if applicable.  Types of respirators to be considered for this material include: 
Organic vapour

For high airborne concentrations, use an approved supplied-air respirator, operated in positive pressure mode.  Supplied air respirators with an escape bottle may be appropriate when oxygen levels are inadequate, gas/vapour warning properties are poor, or if air purifying filter capacity/rating may be exceeded.

Hand Protection:   Any specific glove information provided is based on published literature and glove manufacturer data.  Glove suitability and breakthrough time will differ depending on the specific use conditions. Contact the glove manufacturer for specific advice on glove selection and breakthrough times for your use conditions. Inspect and replace worn or damaged gloves. The types of gloves to be considered for this material include:
Nitrile,Viton
Chemical resistant gloves are recommended. If contact with forearms is likely wear gauntlet style gloves.

Eye Protection:   If contact is likely, safety glasses with side shields are recommended.

Skin and Body Protection:    Any specific clothing information provided is based on published literature or manufacturer data.  The types of clothing to be considered for this material include:
 Chemical/oil resistant clothing is recommended.

Specific Hygiene Measures:   Always observe good personal hygiene measures, such as washing after handling the material and before eating, drinking, and/or smoking. Routinely wash work clothing and protective equipment to remove contaminants. Discard contaminated clothing and footwear that cannot be cleaned. Practise good housekeeping.

ENVIRONMENTAL CONTROLS
 See Sections  6,  7, 12, 13.

SECTION 9	 PHYSICAL AND CHEMICAL PROPERTIES	

Typical physical and chemical properties are given below.   Consult the Supplier in Section 1 for additional data.

GENERAL INFORMATION
Physical State:    Liquid 
Colour:   Clear (May Be Dyed)
Odour:   Petroleum/Solvent
Odour Threshold:   N/D

IMPORTANT HEALTH, SAFETY, AND ENVIRONMENTAL INFORMATION
Relative Density (at 15 C):    0.775 -  0.83   
Flash Point [Method]:     >38C  (100F) [ IP 170/70]
Flammable Limits (Approximate volume % in air):   LEL:  0.7     UEL: 5.0  
Autoignition Temperature:   250°C  (482°F)
Boiling Point / Range:    > 150C  (302F)
Vapour Density (Air = 1):   N/D
Vapour Pressure:   < 0.133 kPa (1 mm Hg) at 20 C
Evaporation Rate (n-butyl acetate = 1):   N/D
pH:   N/A
Log Pow (n-Octanol/Water Partition Coefficient):   > 3.5
Solubility in Water:   Negligible
Viscosity:   1.1 cSt  (1.1 mm2/sec) at 40 C
Oxidizing Properties:  See Hazards Identification Section.

OTHER INFORMATION
Freezing Point:   -47°C  (-53°F)
Melting Point:   N/A       

 SECTION 10	 STABILITY AND REACTIVITY	

STABILITY:  Material is stable under normal conditions.

CONDITIONS TO AVOID:  Avoid heat, sparks, open flames and other ignition sources.

INCOMPATIBLE MATERIALS:   Halogens,  Strong Acids,  Alkalies,  Strong oxidisers

HAZARDOUS DECOMPOSITION PRODUCTS:  Material does not decompose at ambient temperatures.

HAZARDOUS REACTIONS:  Will not occur.

SECTION 11	 TOXICOLOGICAL INFORMATION	

ACUTE TOXICITY

 Route of Exposure	 Conclusion / Remarks	
Inhalation		
Toxicity (Rat): LC50 > 5000 mg/m3	Minimally Toxic. Based on test data for structurally similar materials.	
Irritation: No end point data.	Elevated temperatures or mechanical action may form vapours, mist, or fumes which may be irritating to the eyes, nose, throat, or lungs. Based on assessment of the components.	
		
Ingestion		
Toxicity (Rat): LD50 > 5000 mg/kg	Minimally Toxic. Based on test data for structurally similar materials.	
		
Skin		
Toxicity (Rabbit): LD50 > 5000 mg/kg	Minimally Toxic. Based on test data for structurally similar materials.	
Irritation (Rabbit): Data available.	Irritating to the skin. Based on test data for structurally similar materials.	
		
Eye 		
Irritation (Rabbit): Data available.	May cause mild, short-lasting discomfort to eyes. Based on test data for structurally similar materials.	

CHRONIC/OTHER EFFECTS
             For the product itself:
 Vapour/aerosol concentrations above recommended exposure levels are irritating to the eyes and respiratory tract, may cause headaches, dizziness, anaesthesia, drowsiness, unconsciousness and other central nervous system effects including death.  Small amounts of liquid aspirated into the lungs during ingestion or from vomiting may cause chemical pneumonitis or pulmonary edema.
Contains:
Kerosene:  Carcinogenic in animal tests. Lifetime skin painting tests produced tumours, but the mechanism is due to repeated cycles of skin damage and restorative hyperplasia. This mechanism is considered unlikely in humans where such prolonged skin irritation would not be tolerated. Did not cause mutations in-vitro. Inhalation of vapours did not result in reproductive or developmental effects in laboratory animals. Inhalation of high concentrations in animals resulted in respiratory tract irritation, lung changes and some reduction in lung function. Non-sensitizing in animal tests.  NAPHTHALENE:  Exposure to high concentrations of naphthalene may cause destruction of red blood cells, anemia, and cataracts. Naphthalene caused cancer in laboratory animal studies, but the relevance of these findings to humans is uncertain.
Ethylbenzene:  Caused cancer in laboratory animal studies. The relevance of these findings to humans is uncertain.

Additional information is available by request.
 
IARC Classification:
The following ingredients are cited on the lists below:
 
 Chemical Name	 CAS Number	 List Citations	
 NAPHTHALENE	 91-20-3	 3	

--REGULATORY LISTS SEARCHED--	
 1 = IARC 1	 2 = IARC 2A	 3 = IARC 2B	

 SECTION 12	 ECOLOGICAL INFORMATION	

The information given is based on data available for the material, the components of the material, and similar materials.

ECOTOXICITY   
             Material -- Expected to be toxic to aquatic organisms. May cause long-term adverse effects in the aquatic environment.

MOBILITY 
             More volatile component -- Highly volatile, will partition rapidly to air.  Not expected to partition to sediment and wastewater solids.
             High molecular wt. component -- Low solubility and floats and is expected to migrate from water to the land.  Expected to partition to sediment and wastewater solids. 

PERSISTENCE AND DEGRADABILITY
Biodegradation: 
             Majority of components --  Expected to be inherently biodegradable  
Atmospheric Oxidation: 
             More volatile component -- Expected to degrade rapidly in air

BIOACCUMULATION POTENTIAL 
             Majority of components -- Has the potential to bioaccumulate, however metabolism or physical properties may reduce the bioconcentration or limit bioavailability.

    

ECOLOGICAL DATA
 
Component	Acute Aquatic Toxicity	
NAPHTHALENE	L(E)C50 >0.1 - 1 mg/L	

 
 SECTION 13	 DISPOSAL CONSIDERATIONS	
 
Disposal recommendations based on material as supplied.  Disposal must be in accordance with current applicable laws and regulations, and material characteristics at time of disposal. 

DISPOSAL RECOMMENDATIONS
 Product is suitable for burning in an enclosed controlled burner for fuel value or disposal by supervised incineration at very high temperatures to prevent formation of undesirable combustion products. 
 
 Empty Container Warning Empty Container Warning (where applicable):  Empty containers may contain residue and can be dangerous.  Do not attempt to refill or clean containers without proper instructions.  Empty drums should be completely drained and safely stored until appropriately reconditioned or disposed.  Empty containers should be taken for recycling, recovery, or disposal through suitably qualified or licensed contractor and in accordance with governmental regulations.  DO NOT PRESSURISE, CUT, WELD, BRAZE, SOLDER, DRILL, GRIND, OR EXPOSE SUCH CONTAINERS TO HEAT, FLAME, SPARKS, STATIC ELECTRICITY, OR OTHER SOURCES OF IGNITION.  THEY MAY EXPLODE AND CAUSE INJURY OR DEATH.

 SECTION 14	 TRANSPORT INFORMATION	

LAND (ADG) 
Proper Shipping Name:   KEROSENE
Dangerous Goods Class/Subsidiary Risk:   3 
Hazchem Code:   3[Y]
UN Number:   1223
Packing Group:   III 
Label(s):    3, EHS 

SEA (IMDG) 
Proper Shipping Name:   KEROSENE
Hazard Class & Division:    3
EMS Number:   F-E, S-E
UN Number:   1223
Packing Group:   III
Marine Pollutant:   Yes
Label(s):   3
Transport Document Name:      UN1223, KEROSENE, 3, PG III, (37.8°C c.c.), MARINE POLLUTANT

AIR (IATA) 
Proper Shipping Name:   KEROSENE
Hazard Class & Division:   3 
UN Number:   1223
Packing Group:   III
Label(s) / Mark(s):   3   
Transport Document Name:    UN1223, KEROSENE, 3, PG III

 SECTION 15	 REGULATORY INFORMATION	
 
Material is hazardous as defined by the Approved Criteria for Classifying Hazardous Substances NOHSC:1008.

CLASSIFICATION:   Category 3 Carcinogen.  Harmful.  Irritant. 

Nature of Special Risk:  R40; Limited evidence of a carcinogenic effect.  R65; Harmful: may cause lung damage if swallowed.  R38; Irritating to skin.

SAFETY PHRASE(S):  S2; Keep out of the reach of children.  S23; Do not breathe vapour.  S24; Avoid contact with skin.  S36/37; Wear suitable protective clothing and gloves.  S43; In case of fire use carbon dioxide (CO2), foam, dry chemical, or water fog.  S61; Avoid release to the environment. Refer to special instructions/safety data sheets.  S62; If swallowed, do not induce vomiting: seek medical advice immediately and show this container or label.

Contains:  KEROSENE, NAPHTHALENE   

Product is regulated according to Australian Dangerous Goods Code. 

Poison Schedule number allocated by the Standard for the Uniform Scheduling of Drugs and Poisons (SUSDP) established under the Therapeutic Goods Act.

REGULATORY STATUS AND APPLICABLE LAWS AND REGULATIONS

Complies with the following national/regional chemical inventory requirements:   AICS, IECSC, DSL, EINECS, ENCS, KECI, PICCS, TSCA

 SECTION 16	 OTHER INFORMATION	

KEY TO ABBREVIATIONS AND ACRONYMS:
N/D = Not determined, N/A = Not applicable, STEL = Short-Term Exposure Limit, TWA = Time-Weighted Average

KEY TO THE RISK CODES CONTAINED IN SECTION 2 AND 3 OF THIS DOCUMENT (for information only):
 R20; Harmful by inhalation.
R22; Harmful if swallowed.
R38; Irritating to skin.
R40; Limited evidence of a carcinogenic effect.
R65; Harmful: may cause lung damage if swallowed.

THIS SAFETY DATA SHEET CONTAINS THE FOLLOWING REVISIONS:
 Revision Changes:
Hazard Identification: Health Hazards was modified.
Section 05: Fire Fighting Measures - Unusual Fire Hazards was modified.
Section 11: Skin Irritation Conclusion was modified.
Section 11: Acute Toxicity Table Header was modified.
Section 01: Product Identification Product Name was modified.
Section 09: Colour was modified.
Section 09: Physical State was modified.
Section 11: Ingestion Acute Lethality - Header was modified.
Section 11: Inhalation - Header was modified.
Section 09: Boiling Point ºC(ºF) was modified.
Section 09: Evaporation Rate - Header was modified.
Section 07: Handling and Storage - Handling was modified.
Section 07: Handling and Storage - Storage Phrases was modified.
Hazard Identification: Physical/Chemical Hazard was modified.
Section 07: Precautions was modified.
Section 11: Dermal Lethality Test Data was modified.
Section 11: Oral Lethality Test Data was modified.
Section 11: Inhalation Lethality Test Data was modified.
Section 05: Hazardous Combustion Products was modified.
Section 06: Accidental Release - Spill Management - Water was modified.
Section 09: Flash Point ºC(ºF) was modified.
Section 09: Viscosity was modified.
Section 08: Hand Protection was modified.
Section 15: EU Contains was modified.
Section 15: National Chemical Inventory Listing was modified.
Section 16: Materials Covered was modified.
Section 16: MSN, MAT ID was modified.
Hazard Identification: Hazards Note was modified.
Hazard Identification: Classification was modified.
Section 15: Classification was modified.
Composition: Component Table was modified.
Composition: Component Table was modified.
Section 15: NATURE OF SPECIAL RISK was modified.
Section 08: Hand Protection CEN Standards - AP was modified.
Section 08: Exposure Limits Table was modified.
Section 16: Prepared By was modified.
Section 09: Oxidizing Properties was modified.
Section 11: Tox List Cited Table was modified.
Section 11: Tox Table - Header was modified.
Composition: Australia Hazardous Substance/Dangerous Good Statements - Header was modified.
Section 08: Biological Limits - Table was modified.
Section 12: Environmental component tox table - Component Column - Header was added.
Section 12: Environmental component tox table - Toxicity Column - Header was added.
Section 12: Environmental component tox table was added.
Section 12: Ecological data - Header was added.

  
THIS SDS COVERS THE FOLLOWING MATERIALS:  DUAL PURPOSE KEROSENE  |  DUAL PURPOSE KEROSENE (133108-85)  |  DUAL PURPOSE KEROSENE (STOCK 6574, 889923-85)
 -----------------------------------------------------------------------------------------------------------------------------------------------------
 The information and recommendations contained herein are, to the best of ExxonMobil's knowledge and belief, accurate and reliable as of the date issued.  You can contact ExxonMobil to insure that this document is the most current available from ExxonMobil.  The information and recommendations are offered for the user's consideration and examination.  It is the user's responsibility to satisfy itself that the product is suitable for the intended use.  If buyer repackages this product, it is the user's responsibility to insure proper health, safety and other necessary information is included with and/or on the container.  Appropriate warnings and safe-handling procedures should be provided to handlers and users.  Alteration of this document is strictly prohibited.  Except to the extent required by law, re-publication or retransmission of this document, in whole or in part, is not permitted.  The term, "ExxonMobil" is used for convenience, and may include any one or more of ExxonMobil Chemical Company, Exxon Mobil Corporation, or any affiliates in which they directly of indirectly hold any interest.

 -----------------------------------------------------------------------------------------------------------------------------------------------------
DGN:  2000400XAU  (1017764)
-----------------------------------------------------------------------------------------------------------------------------------------------------
 Prepared by:          Exxon Mobil Corporation
                              EMBSI, Clinton NJ USA
Contact Point:       See Section 1 for Local Contact number

End of (M)SDS